CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Fri Jun  2 14:40:17 2023
Release      : TopSpin 4.2.0
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.2.176.20221013
CPU          : Intel(R) Core(TM) i5-8400H CPU @ 2.50GHz (8 cores at 3900 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 600 NMR spectrometer
1H-frequency : 600.40 MHz
Description  : AV NEO 600
Bruker Order : 5051813
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- SCU: AV4I SCU SYSTEM CONTROL UNIT Z162978/01226 ECL 02.01
- {EPU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/01226 ECL 02.01
- {GTU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/01226 ECL 02.01
  Location: slot 7 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312125813
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd11, RTD at /dev/bbu/rtd4.4, GPROC at /dev/bbu/gproc4.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/08201 ECL 02.06
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx9.5, RTD at /dev/bbu/rtd9.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/08200 ECL 02.06
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.46 via PCIe #11
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd29, DRX at /dev/bbu/drx11.5, RTD at /dev/bbu/rtd11.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/08199 ECL 02.06
  Location: slot 5 in rack 1
  Connection: at IP 192.168.180.54 via PCIe #13
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd38, DRX at /dev/bbu/drx13.5, RTD at /dev/bbu/rtd13.4
  Sequencer: FCube
  - FCube3
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/08198 ECL 02.06
  Location: slot 6 in rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd2, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube4
- PSM-A: AV4 PSM-A Z149510/03288 ECL 04.00
- HPPR/2 COVER2: HPPR/2 Cover2N Z178831/00491 ECL 00.00
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (reflection meter with CRP-Bias capability)
                  PN=Z103205, SN=01568 from 20220622
      Module  2 : 2H
                  PN=Z003473, SN=02169 from 20220429
      Module  3 : HPLNA 1H19F (reflection meter with CRP-Bias capability)
                  PN=Z103205, SN=01567 from 20220622
      Module  4 : 13C/79Br
                  PN=Z003524, SN=01454 from 20220401
      Module  5 : 15N
                  PN=Z003530, SN=01311 from 20220420
  
- HPLNA 1H19F: HPLNA 1H MODULE 600 Z103205/01568 ECL 06.06
- 2H: HPPR/2 2H MODULE 600 Z003473/02169 ECL 07.00
- HPLNA 1H19F: HPLNA 1H MODULE 600 Z103205/01567 ECL 06.06
- 13C/79Br: HPPR/2 13C MODULE 600 Z003524/01454 ECL 08.00
- 15N: HPPR/2 15N MODULE 600 Z003530/01311 ECL 07.01
- RACK: AV4I AQS CHASSIS Z175600/00750 ECL 03.00
- FANTRAY: AV4I AQS FAN TRAY Z175900/00726 ECL 00.00
- PSM-48V: AV4 PSM-48V Z149850/05351 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/03194 ECL 01.02
- REF 1200: AV4 REFERENCE 1200 Z148270/02916 ECL 02.03


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144061-001294 W144061/001294 ECL 30:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABBH500/100 200-600: W144061/001294 ECL 30
- Controller     = BLA CONTROL BOARD 7: W133936/026225 ECL 40
BLA-W144061-001297 W144061/001297 ECL 30:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABBH500/100 200-600: W144061/001297 ECL 30
- Controller     = BLA CONTROL BOARD 7: W133936/026173 ECL 40
LTRX Z109890/01592 ECL 03.02:
- TCP/IP address = 192.168.99.10
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01592 ECL 03.02

BSMS: BSMS/2 functionality available
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20210921
- Note:  The ELCB firmware is too old.
- ELCB = BSMS/2 ELCB: Z100818/09698 ECL 07.03
- SLCB functionality: Available
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS3-SB
- SCB channels = 40
- Shim matrix file: 292722ca.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01592 ECL 03.02
- Lock: On L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/06773 ECL 05.05
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/02660 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 192.168.98.8

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159072/362
- TCP/IP address   = 192.168.98.5

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99

Magnet System: BZH 749'60'70H04_D325-54-11546 Z115312/MSC11546 ECL H
- Magnet  : BZH 749'600'70H
- Cryostat: D325-54-11546
- Polarity: SN (Bruker)


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 2 of transmitter 2 (AV4 BLABBH500/100 200-600 W144061/001297 at TCP/IP 192.168.99.11)
TRX1 AUX  output -> input 1 of transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/01592 at TCP/IP 192.168.99.10)
TRX2 NORM output -> input 2 of transmitter 1 (AV4 BLABBH500/100 200-600 W144061/001294 at TCP/IP 192.168.99.12)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 2 (AV4 BLABBH500/100 200-600 W144061/001297 at TCP/IP 192.168.99.11)
TRX3 AUX  output -> open
TRX4 NORM output -> input 1 of transmitter 1 (AV4 BLABBH500/100 200-600 W144061/001294 at TCP/IP 192.168.99.12)
TRX4 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABBH500/100 200-600 W144061/001294 at TCP/IP 192.168.99.12:
- amplifier B-500W uses blanking 4
- amplifier 1H-100W uses blanking 2

transmitter 2 = AV4 BLABBH500/100 200-600 W144061/001297 at TCP/IP 192.168.99.11:
- amplifier B-500W uses blanking 3
- amplifier 1H-100W uses blanking 1

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/01592 at TCP/IP 192.168.99.10:
- amplifier 2H-5W uses blanking 9


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX1 -> 2H          -> REC1
Tune-TRX2 -> HPLNA 1H19F -> REC2
Tune-TRX3 -> 13C/79Br    -> REC3
Tune-TRX4 -> 15N         -> REC4

